[AL-CX11]
EPWVER="3.01"
DRVNAME="EPSON AL-CX11 Advanced"
MaxCaset=2
PaperNearEnd=19
Messagetype=1
SoundNotifyEnable=0
TrayIconEnable=0
TrayIconSelected=0
TrayIconEndTime=10000

TIMEOUT=60
TimeOutCountConfirmErr=3
TimeOutCount=10
TimeOutCountReadyErr=1
EnableGetStatusErr=1
JobControl=1

HostbaseType=0
Group=2
PopupLimitBit=0
MaxTonerNum=4
MaxLightNum=1
RedStatus=0

SpoolJobVisible = 1
ActiveTab = 1
MonitoringIcon = 1
JobNameChange = 1

[Language]
English=9h

[English]
RESDLL="E_L1E442.DLL"
HELPFILE="E_SMSTE2.HLP"
SHORTCUT="EPSON Status Monitor 3 Environment Check(2)"
SOUND=0
TSS001=0
TSS002=0
TSS003=0
TSS004=0
TSS005=0
TSS006=0
TSS007=0
TSS008=0
TSS009=0
TSS010=0
TSS011=0
TSS012=0
TSS013=0

[Install]
REGPATH=REG1,"HKEY_LOCAL_MACHINE\Software\EPSON\STM3\Driver\EPSON AL-CX11 Advanced"
REGENTER=REG1,"InstallPath",DRIVERDIR
REGENTER=REG1,"ModelID","AL-CX11"
REGENTER=REG1,"E_SRUN",DRIVERDIR+"\E_L19442.EXE"
REGENTER=REG1,"E_SENV",DRIVERDIR+"\E_L19442.EXE"
REGENTER=REG1,"E_SICN",DRIVERDIR+"\E_L17442.EXE"
REGENTER=REG1,"E_STMS",DRIVERDIR+"\E_L19442.EXE"
REGENTER=REG1,"E_SRCV",DRIVERDIR+"\E_SRCV02.EXE"
REGENTER=REG1,"DepExe",DRIVERDIR+"\E_L18442.EXE"
REGENTER=REG1,"E_SMDL",DRIVERDIR+"\E_L15442.DLL"
REGENTER=REG1,"SHORTCUTEXE_R","E_SRCV02.EXE"
REGENTER=REG1,"JobTimer","30,30,20,20:10,10,10,10"
REGENTER=REG1,"SpoolTimer",5

REGENTER=REG1,"EBAPI16","EBAPI16.DLL"
REGENTER=REG1,"EBAPI32","EBAPI.DLL"
REGENTER=REG1,"EBAPISDK","EEBSDKIF.DLL"

REGPATH=REG2,"HKEY_LOCAL_MACHINE\Software\EPSON\STM3\Profile"
REGENTER=REG2,"AL-CX11",DRIVERDIR+"\E_L1X442.DAT"

REGPATH=REG3,"HKEY_LOCAL_MACHINE\Software\EPSON\STM3\STMCommon"

DRVNAME="EPSON AL-CX11 Advanced"
ADDEEBPARAM="/TS"

LANGUAGEMON1="E_SLM401.DLL","EPSON V3 Monitor401"
LANGUAGEMON2="",""
LANGUAGEMON3="E_SL2401.DLL","EPSON V3 2KMonitor401"
SDKFILENAME2="EB_SET04.EXE"
;
SETLPT=ALL    ,"LPT_Channel00"          ,REG_DWORD,268500994
SETLPT=ALL    ,"LPT_ChnlMode00"         ,REG_DWORD,7
SETLPT=ALL    ,"LPT_Channel01"          ,REG_DWORD,268500996
SETLPT=ALL    ,"LPT_ChnlMode01"         ,REG_DWORD,3
SETLPT=ALL    ,"LPT_WriteTotalTimeOut"  ,REG_DWORD,3000
SETLPT=WIN9X  ,"LPT_ReadTotalTimeOut"   ,REG_DWORD,1000
SETLPT=WINNT40,"LPT_ReadTotalTimeOut"   ,REG_DWORD,10000
SETLPT=WIN2000,"LPT_ReadTotalTimeOut"   ,REG_DWORD,10000
SETLPT=ALL    ,"LPT_ReadIntervalTimeOut",REG_DWORD,20
SETLPT=ALL    ,"LPT_PrtMDLName"         ,REG_SZ   ,"AL-CX11"
SETLPT=ALL    ,"LPT_SetTimeOutFlag"     ,REG_DWORD,1
SETLPT=ALL    ,"LPT_StatusLength"       ,REG_DWORD,121
SETLPT=ALL    ,"LPT_DeviceIDReply"		,REG_DWORD,1
;
